Skip to main content.
Related Sites: Home | Project Page | Forum | Docs | SingleClick | CVS

# UltraVNC

Remote Control for all
Tools: download stable version « | download develop version «
Navigation: Home | General | Installation | Features | Add-ons

- Repeater
- NAT2NAT
- Forwarding
- SingleClick

# Port Forwarding with NAT routers

If UltraVNC server and viewer are on different sides of a NAT router and you won't use a repeater or NAT-to-NAT connector, you need to do some configuration on the router.

Here are some links to detailled configuration instructions for specific router types.

A general overview about port forwarding is given in What is Port Forwarding?

## Router configuration

- Port Forwarding: Linksys Cable/DSL Router - Single Ports (1.2x firmware)
- Port Forwarding: Linksys Cable/DSL Router - Port Ranges (1.3x firmware)
- Port Forwarding: D-Link 704P DSL/Cable Router
- Port Forwarding: Asante FR3000 DSL/Cable Router
- Port Forwardingstep-by-step instructions for various manufacturers

## Firewall configuration

- http://www.paulscomputerservice.net/index.php?body=./tutorials/ultravnc.php