Skip to main content.
Related Sites: Home | Project Page | Forum | Docs | SingleClick | CVS

# UltraVNC

Remote Control for all
Tools: download stable version « | download develop version «
Navigation: Home | General | Installation | Features | Add-ons

- Install
- Configure
- Usage
- Cmdline
- Viewer
- Registry
- Unattended

# UltraVNC Configuration

## Admin Properties

The "Admin Properties" menu item in the system tray UltraVNC icon menu referres to Default Local System Properties and allows for customizing several areas:

Incoming connections
  Accept Socket Connections
    Should be activated for normal operation. The display number and ports to use can be configured or set to `Auto` which defaults to Display `0`, Port `5900` and JavaViewer port `5800`.
    The port is always Display No + 5900.
  Display
    Defaults to `0`.
  Ports
    Defaults to `5900` and `5800` for HTTP.
  Enable JavaViewer (HTTP connect)
    Allows to view a remote computer by opening a browser and go to `http://remote-machine:http-port/`
  Allow Loopback Connections
    Sometimes this could be helpful for tests. Normally it's not needed since the result is not very useful.
  Loopback Only
    Needed for tests. Connections from outside are not allowed.
When last client disconnects
  In a helpdesk scenario, you normally "Do Nothing" when disconnecting. When administering servers via remote control, you might wish to either "Lock Workstation" or "Logoff Workstation" for security reasons.
Query on incoming connection
  If enabled, every time someone tries to connect via UltraVNC, a pop-up dialog informs the user and asks the user to either accept or refuse the attempt. Configure the timeout for the dialog window and what action should be taken if the user clicked no button until timeout.
Keyboard & Mouse
  Some situations (e.g. presentations) require that either the viewer or the remote computer don't input keyboard or mouse events. This can be configured by "Disable Viewer inputs" or "Disable Local inputs".
Multi viewer connections
  Here you can configure the behavior if multiple viewers attempt to connect to the same UltraVNC server. "Disconnect all existing connections" implies that only one viewer can be connected at a time and the last one wins. "Keep existing connections" allows for several viewers simultaneously. "Refuse the new connection" implies that only one viewer can be connected at a time and the first one wins. "Refuse all new connections" ??
Authentication
  "VNC Password" is a per-machine password and is required.
  Require MS Logon
    Activates MS-Logon I. Works on Windows 9x as well as Windows NT4/2000/XP. Requires computer and user to be in the same domain.
  New MS Logon
    Activates MS-Logon II. Allows for cross-domain authentication, i.e. computer is in domain A, user in domain B with a trust between A and B (typically in Active Directory). Works only on Windows NT4/2000/XP.
  Configure MS Logon Groups
    opens the configuration dialog for MS-Logon authorization. For MS-Logon I there is a dialog allowing to configure 3 groups.
    For MS-Logon II there is the standard Windows Security property page.
DSM Plugin
  If there are any DSM (Data Stream Modification) Plugins available, their usage can be configured here. Currently there are several encryption plugins available.
Miscellaneous
  Remove Wallpaper for Viewers
    To reduce network traffic the wallpaper on the remote computer's desktop can be removed during the connection.
  Enable Blank Monitor on Viewer Request
    Allow viewers to disable the monitor if they request so.
  Enable File Transfer
    Enable the UltraVNC File Transfer.
  Log debug infos to the WinVNC.log file
    Enable logging. The log file is in C:\WinNT\system32 if winvnc runs as service. The logging level can be configured in the registry.
  Disable TrayIcon
    The icon in the system tray can be disabled to disallow users to change any settings.
  Forbid the user to close down WinVNC
    Disallow users to close down WinVNC.
  Disable clients options in tray icon menu
    Disable the "Properties" menu item in the system tray icon menu.
  Capture Alpha-Blending
    ??
  Enable Alpha-Blending Screen Blanking
    Enable another method to disable the monitor.
  Default Server Screen Scale
    The server screen can be scaled down here.

## Properties

The "Properties" menu item in the system tray UltraVNC icon menu referres to per user settings.

Poll Full Screen
  ??
Poll Foreground Window
  ??
Poll Console Windows Only
  ??
Poll Window Under Cursor
  ??
Poll On Event Only
  ??
System Hook Dll
  Provides DDI hooking, especially on Windows 9x.
Video Hook Driver
  The video hook driver provides high speed and low CPU load on Windows 2000/XP/2003.
Check the Video Hook Driver
  Here you can test the video hook driver, see it's version and whether it's currently active.
Low Accuracy
  Get higher speed with reduced accuracy.
Share only the Server Window Named
  Do not share the whole desktop but only the window with the specified name.